- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Fields

# binary_stream Struct Reference
[NPF driver internals manual]

A stream of X86 binary code. More...

`#include <jitter.h>`

## Data Fields
INT | cur_ip
| Current X86 instruction pointer.
INT | bpf_pc
| Current BPF instruction pointer, i.e. position in the BPF program reached by the jitter.
PCHAR | ibuf
| Instruction buffer, contains the X86 generated code.
PUINT | refs
| Jumps reference table.

## Detailed Description

A stream of X86 binary code.

Definition at line 65 of file jitter.h.

## Field Documentation

INT cur_ip

Current X86 instruction pointer.

Definition at line 66 of file jitter.h.

INT bpf_pc

Current BPF instruction pointer, i.e. position in the BPF program reached by the jitter.

Definition at line 67 of file jitter.h.

PCHAR ibuf

Instruction buffer, contains the X86 generated code.

Definition at line 68 of file jitter.h.

PUINT refs

Jumps reference table.

Definition at line 69 of file jitter.h.

The documentation for this struct was generated from the following file:

- jitter.h

documentation. Copyright (c) 2002-2005 Politecnico di Torino. Copyright (c) 2005-2007 CACE Technologies. All rights reserved.