ENTER mysub_SessionManager_CMD_RECV_Process_00788E80
Session ID=0 
Session CMD=44
ENTER: mysub_call_on_reply_check_possible_Flush_decode_pkt_header_decode_fail
ENTER unpack_7_bit_encoded_to_dword 
LEAVE unpack_7_bit_encoded_to_dword 
First INT:B
ENTER mysub_local_realloc_alloc_getlast_err_exception
LEAVE mysub_local_realloc_alloc_getlast_err_exception
ENTER copy_memory1
LEAVE copy_memory1
ENTER mysub_no_call_00724060
LEAVE mysub_no_call_00724060
ENTER copy_memory2
COPY_MEMORY2: ecx=0x00000005 esi=0x0012F2A4
LEAVE copy_memory2
ENTER mysub_call_eax__free()
LEAVE mysub_call_eax__free()
ENTER mysub_unpack_7_bit_encoded
heap_alloc_buf=3207A8,var5=3207A8
1:READ BYTE7b=0
ENTER unpack_7_bit_encoded_to_dword___2
READ BYTE=3
ecx=3
LEAVE unpack_7_bit_encoded_to_dword___2
MAINBUF 2: size(0x00000014)
00000000 00000003 00000000 00000000 | 00000000 
IF: eax=0,ebp=0
ENTER unpack_7_bit_encoded_to_dword___2
READ BYTE=D8
ecx=58
READ BYTE=4C
ecx=2658
LEAVE unpack_7_bit_encoded_to_dword___2
MAINBUF 3: size(0x00000014)
00000000 00000003 00002658 00000000 | 00000000 
LEAVE mysub_unpack_7_bit_encoded
ENTER copy_memory1
LEAVE copy_memory1
ENTER mysub_no_call_00724060
LEAVE mysub_no_call_00724060
ENTER copy_memory2
COPY_MEMORY2: ecx=0x00000005 esi=0x0012F2A4
LEAVE copy_memory2
ENTER mysub_call_eax__free()
LEAVE mysub_call_eax__free()
ENTER mysub_unpack_7_bit_encoded
heap_alloc_buf=3207A8,var5=3207BC
1:READ BYTE7b=4
ENTER unpack_7_bit_encoded_to_dword___2
READ BYTE=1
ecx=1
LEAVE unpack_7_bit_encoded_to_dword___2
MAINBUF 2: size(0x00000028)
00000000 00000003 00002658 00000000 | 00000000 00000004 00000001 00000000 
00000000 00000000 
IF: eax=4,ebp=0
ENTER unpack_7_bit_encoded_to_dword___2
READ BYTE=15
ecx=15
LEAVE unpack_7_bit_encoded_to_dword___2
MAINBUF 5: size(0x00000028)
00000000 00000003 00002658 00000000 | 00000000 00000004 00000001 00000000 
00000000 00000015 
ENTER mysub_local_alloc_memerr_exception
str alloc size:0x00000015
LEAVE mysub_local_alloc_memerr_exception
ENTER copy_memory2
COPY_MEMORY2: ecx=0x00000005 esi=0x0042B0C7
LEAVE copy_memory2
3.1: size(0x00000015)
BAA19719 A6C4F0C6 01C0A801 1CB33943 | A2AD8F7D 48000000 
ENTER copy_memory1
LEAVE copy_memory1
ENTER mysub_no_call_00724060
LEAVE mysub_no_call_00724060
ENTER copy_memory2
COPY_MEMORY2: ecx=0x00000005 esi=0x0012F2A4
LEAVE copy_memory2
ENTER mysub_call_eax__free()
LEAVE mysub_call_eax__free()
ENTER mysub_unpack_7_bit_encoded
heap_alloc_buf=3207A8,var5=3207D0
1:READ BYTE7b=1
ENTER unpack_7_bit_encoded_to_dword___2
READ BYTE=9
ecx=9
LEAVE unpack_7_bit_encoded_to_dword___2
MAINBUF 2: size(0x0000003C)
00000000 00000003 00002658 00000000 | 00000000 00000004 00000001 00000000 
00320A60 00000015 00000001 00000009 | 00000000 00000000 00000000 
IF: eax=1,ebp=0
perviy int = 1










eax=0x0000004C
edx=0x00000000
eax=0x0000004C
edx=0x00000000




eax=0x00000091
edx=0x00000000
eax=0x00000091
edx=0x00000000




eax=0x00000020
edx=0x00000000
eax=0x00000020
edx=0x00000000




eax=0x0000003A
edx=0x00000000
eax=0x0000003A
edx=0x00000000


ENTER copy_memory1
LEAVE copy_memory1
ENTER mysub_no_call_00724060
LEAVE mysub_no_call_00724060
ENTER copy_memory2
COPY_MEMORY2: ecx=0x00000005 esi=0x0012F2A4
LEAVE copy_memory2
ENTER mysub_call_eax__free()
LEAVE mysub_call_eax__free()
ENTER mysub_unpack_7_bit_encoded
heap_alloc_buf=3207A8,var5=3207E4
1:READ BYTE7b=0
ENTER unpack_7_bit_encoded_to_dword___2
READ BYTE=1B
ecx=1B
LEAVE unpack_7_bit_encoded_to_dword___2
MAINBUF 2: size(0x00000050)
00000000 00000003 00002658 00000000 | 00000000 00000004 00000001 00000000 
00320A60 00000015 00000001 00000009 | 00000000 4C91203A F45CA4FF 00000000 
0000001B 00000000 00000000 00000000 | 
IF: eax=0,ebp=0
ENTER unpack_7_bit_encoded_to_dword___2
READ BYTE=6
ecx=6
LEAVE unpack_7_bit_encoded_to_dword___2
MAINBUF 3: size(0x00000050)
00000000 00000003 00002658 00000000 | 00000000 00000004 00000001 00000000 
00320A60 00000015 00000001 00000009 | 00000000 4C91203A F45CA4FF 00000000 
0000001B 00000006 00000000 00000000 | 
LEAVE mysub_unpack_7_bit_encoded
ENTER copy_memory1
LEAVE copy_memory1
ENTER mysub_no_call_00724060
LEAVE mysub_no_call_00724060
ENTER copy_memory2
COPY_MEMORY2: ecx=0x00000005 esi=0x0012F2A4
LEAVE copy_memory2
ENTER mysub_call_eax__free()
LEAVE mysub_call_eax__free()
ENTER mysub_unpack_7_bit_encoded
heap_alloc_buf=3207A8,var5=3207F8
1:READ BYTE7b=5
ENTER unpack_7_bit_encoded_to_dword___2
READ BYTE=7
ecx=7
LEAVE unpack_7_bit_encoded_to_dword___2
MAINBUF 2: size(0x00000064)
00000000 00000003 00002658 00000000 | 00000000 00000004 00000001 00000000 
00320A60 00000015 00000001 00000009 | 00000000 4C91203A F45CA4FF 00000000 
0000001B 00000006 00000000 00000000 | 00000005 00000007 00000000 00000000 
00000000 
IF: eax=5,ebp=0
ENTER mysub_local_alloc_memerr_exception
str alloc size:0x00000010
LEAVE mysub_local_alloc_memerr_exception
ENTER: mysub_call_on_reply_check_possible_Flush_decode_pkt_header_decode_fail
ENTER unpack_7_bit_encoded_to_dword 
LEAVE unpack_7_bit_encoded_to_dword 
First INT:3
ENTER mysub_local_realloc_alloc_getlast_err_exception
LEAVE mysub_local_realloc_alloc_getlast_err_exception
ENTER copy_memory1
LEAVE copy_memory1
ENTER mysub_no_call_00724060
LEAVE mysub_no_call_00724060
ENTER copy_memory2
COPY_MEMORY2: ecx=0x00000005 esi=0x0012F2A4
LEAVE copy_memory2
ENTER mysub_call_eax__free()
LEAVE mysub_call_eax__free()
ENTER mysub_unpack_7_bit_encoded
heap_alloc_buf=320AF0,var5=320AF0
1:READ BYTE7b=2
ENTER unpack_7_bit_encoded_to_dword___2
READ BYTE=8
ecx=8
LEAVE unpack_7_bit_encoded_to_dword___2
MAINBUF 2: size(0x00000014)
00000002 00000008 00000000 00000000 | 00000000 
IF: eax=2,ebp=0
perviy int = 1










eax=0x000000DA
edx=0x00000000
eax=0x000000DA
edx=0x00000000




eax=0x00000025
edx=0x00000000
eax=0x00000025
edx=0x00000000




eax=0x00000000
edx=0x00000000
eax=0x00000000
edx=0x00000000




eax=0x00000003
edx=0x00000000
eax=0x00000003
edx=0x00000000


ENTER copy_memory1
LEAVE copy_memory1
ENTER mysub_no_call_00724060
LEAVE mysub_no_call_00724060
ENTER copy_memory2
COPY_MEMORY2: ecx=0x00000005 esi=0x0012F2A4
LEAVE copy_memory2
ENTER mysub_call_eax__free()
LEAVE mysub_call_eax__free()
ENTER mysub_unpack_7_bit_encoded
heap_alloc_buf=320AF0,var5=320B04
1:READ BYTE7b=DC
ENTER unpack_7_bit_encoded_to_dword___2
READ BYTE=AC
ecx=2C
READ BYTE=1
ecx=AC
LEAVE unpack_7_bit_encoded_to_dword___2
MAINBUF 2: size(0x00000028)
00000002 00000008 00000000 DA250003 | 4E748A5F 000000DC 000000AC 00000000 
00000000 00000000 
IF: eax=DC,ebp=0
perviy int != 4 (new unknown case), hz 29, eax=0x000000DC
error code 0 returned after mysub_unpack_7_bit_encoded, hz 21
error code 0 returned after mysub_unpack_7_bit_encoded, hz 21
Flush_decode.. call fail with ret=0, jump on hzkuda4
decode failed
decode 41 failed
