- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

# wpcap_remote.htm

Go to the documentation of this file.

    00001 <html>
    00002
    00003 <head>
    00004 <meta http-equiv="Content-Type" content="text/html; charset=windows-1252">
    00005 <meta name="GENERATOR" content="Microsoft FrontPage 4.0">
    00006 <meta name="ProgId" content="FrontPage.Editor.Document">
    00007 <title>Using WinPcap Remote Capture</title>
    00008 </head>
    00009
    00010 <body>
    00011
    00012 <hr>
    00013 <ul>
    00014   <li><a href="#RunningModes">Remote Capture Running Modes</a></li>
    00015   <li><a href="#Config">Configuring the Remote Daemon (rpcapd)</a></li>
    00016   <li><a href="#StartCap">Starting a capture on a remote machine</a></li>
    00017   <li><a href="#UNIX">Installing the Remote Capture Daemon in UNIX</a></li>
    00018 </ul>
    00019 <hr>
    00020 <p>WinPcap comes with Remote Capture capabilities. This is an highly
    00021 experimental feature that allows to interact to a remote machine and capture
    00022 packets that are being transmitted on the remote network.</p>
    00023 <p>This requires a <b>remote daemon </b>(called <code>rpcapd</code>) which
    00024 performs the capture and sends data back and a <b>local client </b>that sends
    00025 the appropriate commands and receives the captured data.</p>
    00026 <p>WinPcap extends the standard WinPcap code in such a way that all
    00027 WinPcap-based tools can expoit remote capture capabilities. For instance, the
    00028 capabillity to interact with a remote daemon are added to the client software
    00029 without any explicit modification to it. Vice versa, the remote daemon must be
    00030 explicitely installed (and configured) on the remote machine.</p>
    00031 <h2><a name="RunningModes"></a>Remote Capture Running Modes</h2>
    00032 <p>The Remote Capture Protocol (RPCAP) can work in two modes:</p>
    00033 <ul>
    00034   <li><b>Passive Mode</b> (default): the client (e.g. a network sniffer)
    00035     connects to the remote daemon, it sends them the appropriate commands, and
    00036     it starts the capture.</li>
    00037   <li><b>Active Mode</b>: the remote daemon try to establish a connection toward
    00038     the client (e.g. the network sniffer); then, the client sends the
    00039     appropriate commands to the daemon and it starts the capture. This name is
    00040     due to the fact thet the daemon becomes <i>active</i> instead of <i>waiting</i>
    00041     for new connections.</li>
    00042 </ul>
    00043 <p>The Active Mode is useful in case the remote daemon is behind a firewall and
    00044 it cannot receive connections from the external world. In this case, the daemon
    00045 can be configured to establish the connection to a given host, which will have
    00046 been configured in order to <i>wait</i> for that connection. After establishing
    00047 the connection, the protocol continues its job in almost the same way in both
    00048 Active and Passive Mode.</p>
    00049 <p>Analyzer (<a href="http://analyzer.polito.it/30alpha/">http://analyzer.polito.it/30alpha/</a>)
    00050 has a set of commands (in the <b>Capture</b> menu) that allows you to accept a
    00051 remote connection and then start the capture on the remote device. Currently,
    00052 Analyzer is the only tool that is able to work in active mode, since it requires
    00053 some modifications to the application code.</p>
    00054 <h2><a name="Config"></a>Configuring the Remote Daemon (rpcapd)</h2>
    00055 <p>The Remote Daemon is a standard Win32 executable running either in console
    00056 mode or as a service. The executable can be found in the <code>WinPcap</code>
    00057 folder and it has the following syntax:</p>
    00058 <pre>        rpcapd [-b &lt;address&gt;] [-p &lt;port&gt;] [-6] [-l &lt;host_list&gt;] [-a &lt;host,port&gt;]
    00059                [-n] [-v] [-d] [-s &lt;file&gt;] [-f &lt;file&gt;]</pre>
    00060 <p>The daemon can be compiled and it is actually working on Linux as well.</p>
    00061 <p>Here there is a brief description of the allowed commands:</p>
    00062 <div align="left">
    00063   <table border="1">
    00064     <tr>
    00065       <th>Switch</th>
    00066       <th>Description</th>
    00067     </tr>
    00068     <tr>
    00069       <td>
    00070         <pre>-b &lt;address&gt;</pre>
    00071       </td>
    00072       <td>It sets the address the daemon has to bind to (either numeric or
    00073         literal). Default: it binds to all local IPv4 and IPv6 addresses.</td>
    00074     </tr>
    00075     <tr>
    00076       <td>
    00077         <pre>-p &lt;port&gt;</pre>
    00078       </td>
    00079       <td>It sets the port the daemon has to bind to. Default: it binds to port
    00080         2002.</td>
    00081     </tr>
    00082     <tr>
    00083       <td>
    00084         <pre>-4</pre>
    00085       </td>
    00086       <td>It binds only to IPv4 addresses. Default: both IPv4 and IPv6 waiting
    00087         sockets are used.</td>
    00088     </tr>
    00089     <tr>
    00090       <td>
    00091         <pre>-l &lt;host_list_file&gt;</pre>
    00092       </td>
    00093       <td>It specifies a file that keeps the list of the hosts which are allowed
    00094         to connect to this daemon (if more than one, the file keeps them one per
    00095         line). We suggest to use literal names (instead of numeric ones) in
    00096         order to avoid problems with different address families (IPv4 and IPv6).</td>
    00097     </tr>
    00098     <tr>
    00099       <td>
    00100         <pre>-n</pre>
    00101       </td>
    00102       <td>It permits NULL authentication (usually used with '-l', that
    00103         guarantees that only the allowed hosts can connect to the daemon).
    00104         Default: the username/password authentication mechanism is required.</td>
    00105     </tr>
    00106     <tr>
    00107       <td>
    00108         <pre>-a &lt;host, port&gt;</pre>
    00109       </td>
    00110       <td>It forces the daemon to run in active mode and to connect to 'host' on
    00111         port 'port'. This does not exclude that the daemon is still able to
    00112         accept passive connections.</td>
    00113     </tr>
    00114     <tr>
    00115       <td>
    00116         <pre>-v</pre>
    00117       </td>
    00118       <td>It forces the daemon to run in active mode only (default: the daemon
    00119         always accepts active connections, even if the '-a' switch is
    00120         specified).</td>
    00121     </tr>
    00122     <tr>
    00123       <td>
    00124         <pre>-d</pre>
    00125       </td>
    00126       <td>Forces the daemon to run in background, i.e. as a daemon (UNIX only)
    00127         or as a service (Win32 only). <b>Warning</b> (Win32): this switch is
    00128         provided automatically when WinPcap installs this daemon into the Win32
    00129         services (control panel - administrative tools - services).</td>
    00130     </tr>
    00131     <tr>
    00132       <td>
    00133         <pre>-s &lt;file&gt;</pre>
    00134       </td>
    00135       <td>It saves the current configuration to file.</td>
    00136     </tr>
    00137     <tr>
    00138       <td>
    00139         <pre>-f &lt;file&gt;</pre>
    00140       </td>
    00141       <td>It loads the current configuration from file; all the switches
    00142         specified from the command line are ignored and the file settings are
    00143         used instead.</td>
    00144     </tr>
    00145     <tr>
    00146       <td>
    00147         <pre>-h</pre>
    00148       </td>
    00149       <td>It prints an help screen.</td>
    00150     </tr>
    00151   </table>
    00152 </div>
    00153 <h3>Installing the remote daemon</h3>
    00154 <p>The remote daemon is installed automatically when installing WinPcap. The
    00155 installation process places the <code>rpcapd</code> file into the <code>WinPcap</code>
    00156 folder. This file can be executed either from the command line, or as a service.
    00157 For instance, the installation process updates the list of available services
    00158 list and it creates a new item (<b>Remote Packet Capture Protocol v.0
    00159 (experimental)</b> ). To avoid security problems, the service is inactive and it
    00160 has to be started manually (control panel - administrative tools - services -
    00161 start).</p>
    00162 <p>The service has a set of &quot;standard&quot; parameters, i.e. it it launched
    00163 with the &quot;<code>-d</code>&quot; flag (in orde to make it running as a
    00164 service) and the &quot;<code>-f rpcapd.ini</code>&quot; flag. The user can
    00165 create a file called <code>rpcapd.ini</code> in the same folder of the
    00166 executable, and put the configuration commands in there. In order for the
    00167 service to execute the commands, you have to stop and restart it again (i.e. the
    00168 initialization file is parsed only at the beginning). Viceversa, the UNIX
    00169 version of <code>rpcapd</code> is able to read the configuration file when
    00170 sending a kill -HUP signal to it. In that case, all the existing connections
    00171 remain in place, while the new connections will be created according to the new
    00172 parameters.</p>
    00173 <p>In case the user does not want to create the configuration file manually, it
    00174 can launch <code>rpcapd</code> with the requested parameters plus the &quot;<code>-s
    00175 filename</code>&quot; one. The daemon will parse all the parameters and save
    00176 them into the specified configuration file.</p>
    00177 <h3>Starting the remote daemon as a standard executable</h3>
    00178 <p>The <code>rpcapd</code> executable can be launched directly, i.e. it can run
    00179 in the foreground as well (not as a daemon/service). The procedure is quite
    00180 simple: you have to invoke the executable from the command line with all the
    00181 requested parameters but the &quot;<code>-d</code>&quot; flag. The capture
    00182 server will start in the foreground.</p>
    00183 <h2><a name="StartCap"></a>Starting a capture on a remote machine</h2>
    00184 <p>If you are using a tool that is already aware of the remote capture (like
    00185 Analyzer), everything is simple. The capture wizard will help you to locate the
    00186 appropriate interface on the remote machine.</p>
    00187 <p>If your preferred tool is not aware of the remote capture, you can still use
    00188 the remote capture. In this case you have to read the next Section.</p>
    00189 <p><b>Be carefully</b>: the capture server (<code>rpcapd</code>) must be up and
    00190 running on the remote machine.</p>
    00191 <h3>New string specifiers for interface selection</h3>
    00192 <p>If your preferred tool is not aware of the remote capture, the only thing you
    00193 must do is to insert, as interface specifier, the indication of the remote
    00194 machine you want to contact. The following forms are allowed:</p>
    00195 <div align="left">
    00196   <table border="1">
    00197     <tr>
    00198       <th>Adapter String</th>
    00199       <th>Description</th>
    00200     </tr>
    00201     <tr>
    00202       <td>
    00203         <pre>file://filename</pre>
    00204       </td>
    00205       <td>It opens a local file.</td>
    00206     </tr>
    00207     <tr>
    00208       <td>
    00209         <pre>rpcap://host.foo.bar/adaptername</pre>
    00210       </td>
    00211       <td>It opens a remote adapter; the host is specified by means of the
    00212         literal name, without port number (i.e. it uses the RPCAP default port).</td>
    00213     </tr>
    00214     <tr>
    00215       <td>
    00216         <pre>rpcap://host.foo.bar:1234/adaptername</pre>
    00217       </td>
    00218       <td>It is the same as before, but it uses a different port number.</td>
    00219     </tr>
    00220     <tr>
    00221       <td>
    00222         <pre>rpcap://10.11.12.13/adaptername</pre>
    00223       </td>
    00224       <td>It opens a remote adapter, but the host is specified by means of an
    00225         IPv4 numeric address, without port number (i.e. it uses the RPCAP
    00226         default port).</td>
    00227     </tr>
    00228     <tr>
    00229       <td>
    00230         <pre>rpcap://10.11.12.13:1234/adaptername</pre>
    00231       </td>
    00232       <td>It is the same as before, but it uses a different port number.</td>
    00233     </tr>
    00234     <tr>
    00235       <td>
    00236         <pre>rpcap://[10.11.12.13]:1234/adaptername</pre>
    00237       </td>
    00238       <td>It is the same as before, but the numeric address is specified within
    00239         square brackets (like IPv6 addresses).</td>
    00240     </tr>
    00241     <tr>
    00242       <td>
    00243         <pre>rpcap://[1:2:3::4]/adaptername</pre>
    00244       </td>
    00245       <td>It opens a remote adapter, but the host is specified by means of an
    00246         IPv6 numeric address, without port number (i.e. it uses the RPCAP
    00247         default port). In case of IPv6 addresses you MUST use the square
    00248         brackets.</td>
    00249     </tr>
    00250     <tr>
    00251       <td>
    00252         <pre>rpcap://[1:2:3::4]:1234/adaptername</pre>
    00253       </td>
    00254       <td>It is the same as before, but it uses a different port number.</td>
    00255     </tr>
    00256     <tr>
    00257       <td>
    00258         <pre>rpcap://adaptername</pre>
    00259       </td>
    00260       <td>It opens a local adapter, without using the RPCAP protocol.</td>
    00261     </tr>
    00262     <tr>
    00263       <td>
    00264         <pre>adaptername</pre>
    00265       </td>
    00266       <td>It opens a local adapter; it is kept for compability, but it is
    00267         strongly discouraged.</td>
    00268     </tr>
    00269     <tr>
    00270       <td>
    00271         <pre>(NULL)</pre>
    00272       </td>
    00273       <td>It opens the first local adapter; it is kept for compability, but it
    00274         is strongly discouraged.</td>
    00275     </tr>
    00276   </table>
    00277 </div>
    00278 <p>The following formats are not allowed:</p>
    00279 <table border="1">
    00280   <tr>
    00281     <th>Adapter String</th>
    00282     <th>Description</th>
    00283   </tr>
    00284   <tr>
    00285     <td>
    00286       <pre>rpcap://</pre>
    00287     </td>
    00288     <td>It cannot be used to open the first local adapter.</td>
    00289   </tr>
    00290   <tr>
    00291     <td>
    00292       <pre>rpcap://hostname/</pre>
    00293     </td>
    00294     <td>It cannot be used to open the first remote adapter.</td>
    00295   </tr>
    00296 </table>
    00297 <h2><a name="UNIX"></a>Installing the Remote Capture Daemon in UNIX</h2>
    00298 <p>The WinPcap source archive can be compiled in UNIX as well. Currently, remote
    00299 capture has been tested on Linux and BSD. What you have to do is:</p>
    00300 <ul>
    00301   <li>download the WinPcap sources</li>
    00302   <li>unpack the sources
    00303     <ul>
    00304       <li>we suggest to use the <code>unzip -a</code> command in order to
    00305         convert DOS files to UNIX ones</li>
    00306     </ul>
    00307   </li>
    00308   <li>move to the <code>libpcap</code> folder</li>
    00309   <li>type:
    00310     <ul>
    00311       <li><code>./configure</code></li>
    00312       <li><b>Warning</b>: in case the previous step reports an error, please
    00313         regenerate the <code>configure</code> file using <code>automake</code>
    00314         (version 2.50 or higher required)</li>
    00315       <li><code>make</code></li>
    00316     </ul>
    00317   </li>
    00318   <li>move to the <code>rpcapd</code> folder</li>
    00319   <li>type <code>make</code></li>
    00320 </ul>
    00321 <p>The remote capture capabilities are turned on by default on Linux and
    00322 FreeBSD. In case you do not want remote capture capabilities in libpcap, you can
    00323 type</p>
    00324 <pre>    ./configure --disable-remote</pre>
    00325 <p>at the &quot;<code>configure</code>&quot; step. All the possible flags are
    00326 listed when typing <code>./configure --help</code>.</p>
    00327 <p>What you obtained right now, is:</p>
    00328 <ul>
    00329   <li>a library file (<code>libpcap.a</code>), which can be linked to other
    00330     applications (like <code>tcpdump</code>) in order to enable the remote
    00331     capture for them.</li>
    00332   <li>an executable (<code>rpcapd</code>) that is the remote daemon</li>
    00333 </ul>
    00334 <p><b>Warning</b>: in order to run the <code>rpcapd</code> daemon, the program
    00335 must either</p>
    00336 <ul>
    00337   <li>run as root (or)</li>
    00338   <li>run as user, but it must be owned by root and must be SUID root (<code>chmod
    00339     u+s rpcapd</code>)</li>
    00340 </ul>
    00341 <h3>Known bugs</h3>
    00342 <p><b>FreeBSD</b>: the first time you call the <code>pcap_stat()</code>, the
    00343 function takes several seconds to return. Therefore, programs like Analyzer seem
    00344 to hang up for 20-30 seconds at the beginning of the capture (if this is done
    00345 with BSD as a remote probe). We're investigating to solve this issue.</p>
    00346 <p><i>For any question, please refer to the WinPcap help page.</i></p>
    00347
    00348 </body>
    00349
    00350 </html>

documentation. Copyright (c) 2002-2005 Politecnico di Torino. Copyright (c) 2005-2007 CACE Technologies. All rights reserved.