BLOBs setup1pkt encoded successfully
BLOBs setup2pkt encoded successfully
BLOBs sess1pkt1 encoded successfully
BLOBs sess1pkt2 encoded successfully
BLOBs sess2pkt1 encoded successfully
BLOBs sess2pkt2 encoded successfully
BLOBs sess2pkt3 encoded successfully
BLOBs sess2pkt3 encoded successfully
BLOBs sess2pkt4 encoded successfully
BLOBs sess3pkt1 encoded successfully
BLOBs sess3pkt2 encoded successfully
BLOBs sess3pkt3 encoded successfully
BLOBs sess3pkt4 encoded successfully
ENTER mysub_SessionManager_CMD_RECV_Process_00788E80
calc sess_id, readed byte: edx=0xFFFFFFFC
calc sess_id, readed byte: edx=0x0000006D
Session ID=36FC 
Session CMD=6D
ENTER: mysub_call_on_reply_check_possible_Flush_decode_pkt_header_decode_fail
ENTER unpack_7_bit_encoded_to_dword 
LEAVE unpack_7_bit_encoded_to_dword 
First INT:3
ENTER mysub_local_realloc_alloc_getlast_err_exception
LEAVE mysub_local_realloc_alloc_getlast_err_exception
ENTER copy_memory1
LEAVE copy_memory1
ENTER mysub_no_call_00724060
LEAVE mysub_no_call_00724060
ENTER copy_memory2
COPY_MEMORY2: ecx=0x00000005 esi=0x0012E244
LEAVE copy_memory2
ENTER mysub_call_eax__free()
LEAVE mysub_call_eax__free()
ENTER mysub_unpack_7_bit_encoded
heap_alloc_buf=3207A8,var5=3207A8
1:READ BYTE7b=0
ENTER unpack_7_bit_encoded_to_dword___2
READ BYTE=1
ecx=1
LEAVE unpack_7_bit_encoded_to_dword___2
MAINBUF 2: size(0x00000014)
00000000 00000001 00000000 00000000 | 00000000 
IF: eax=0,ebp=0
ENTER unpack_7_bit_encoded_to_dword___2
READ BYTE=87
ecx=7
READ BYTE=BF
ecx=1F87
READ BYTE=86
ecx=19F87
READ BYTE=AC
ecx=5819F87
READ BYTE=5
ecx=55819F87
LEAVE unpack_7_bit_encoded_to_dword___2
MAINBUF 3: size(0x00000014)
00000000 00000001 55819F87 00000000 | 00000000 
LEAVE mysub_unpack_7_bit_encoded
ENTER copy_memory1
LEAVE copy_memory1
ENTER mysub_no_call_00724060
LEAVE mysub_no_call_00724060
ENTER copy_memory2
COPY_MEMORY2: ecx=0x00000005 esi=0x0012E244
LEAVE copy_memory2
ENTER mysub_call_eax__free()
LEAVE mysub_call_eax__free()
ENTER mysub_unpack_7_bit_encoded
heap_alloc_buf=3207A8,var5=3207BC
1:READ BYTE7b=0
ENTER unpack_7_bit_encoded_to_dword___2
READ BYTE=3
ecx=3
LEAVE unpack_7_bit_encoded_to_dword___2
MAINBUF 2: size(0x00000028)
00000000 00000001 55819F87 00000000 | 00000000 00000000 00000003 00000000 
00000000 00000000 
IF: eax=0,ebp=0
ENTER unpack_7_bit_encoded_to_dword___2
READ BYTE=2
ecx=2
LEAVE unpack_7_bit_encoded_to_dword___2
MAINBUF 3: size(0x00000028)
00000000 00000001 55819F87 00000000 | 00000000 00000000 00000003 00000002 
00000000 00000000 
LEAVE mysub_unpack_7_bit_encoded
ENTER copy_memory1
LEAVE copy_memory1
ENTER mysub_no_call_00724060
LEAVE mysub_no_call_00724060
ENTER copy_memory2
COPY_MEMORY2: ecx=0x00000005 esi=0x0012E244
LEAVE copy_memory2
ENTER mysub_call_eax__free()
LEAVE mysub_call_eax__free()
ENTER mysub_unpack_7_bit_encoded
heap_alloc_buf=3207A8,var5=3207D0
1:READ BYTE7b=0
ENTER unpack_7_bit_encoded_to_dword___2
READ BYTE=8
ecx=8
LEAVE unpack_7_bit_encoded_to_dword___2
MAINBUF 2: size(0x0000003C)
00000000 00000001 55819F87 00000000 | 00000000 00000000 00000003 00000002 
00000000 00000000 00000000 00000008 | 00000000 00000000 00000000 
IF: eax=0,ebp=0
ENTER unpack_7_bit_encoded_to_dword___2
READ BYTE=1
ecx=1
LEAVE unpack_7_bit_encoded_to_dword___2
MAINBUF 3: size(0x0000003C)
00000000 00000001 55819F87 00000000 | 00000000 00000000 00000003 00000002 
00000000 00000000 00000000 00000008 | 00000001 00000000 00000000 
LEAVE mysub_unpack_7_bit_encoded
LEAVE: mysub_call_on_reply_check_possible_Flush_decode_pkt_header_decode_fail
last bytes ( 0x5D 0x80 0x00 0x00 )
left=0x00000004 buflen=0x00000016
MAINBUF COMPLETED: size(0x0000003C)
00000000 00000001 55819F87 00000000 | 00000000 00000000 00000003 00000002 
00000000 00000000 00000000 00000008 | 00000001 00000000 00000000 
no alloc struct-esLEAVE mysub_SessionManager_CMD_RECV_Process_00788E80
possible not all bytes decoded! (not found last 2 bytes of crc16)
==============================================
PKT:
==============================================
Session id:  0x000036FC (14076)
Session cmd: 0x0000006D (109)
MAIN: size(0x0000003C)
00000000 00000001 55819F87 00000000 | 00000000 00000000 00000003 00000002 
00000000 00000000 00000000 00000008 | 00000001 00000000 00000000 

next bytes: 0x00000000 0x00000001 0x55819F87 0x00000000 0x00000000 
obj_type :  0x00000000
obj_index:  0x00000001
data:       0x55819F87
data_ptr:   0x00000000 0x00000000

next bytes: 0x00000000 0x00000003 0x00000002 0x00000000 0x00000000 
obj_type :  0x00000000
obj_index:  0x00000003
data:       0x00000002
data_ptr:   0x00000000 0x00000000

next bytes: 0x00000000 0x00000008 0x00000001 0x00000000 0x00000000 
obj_type :  0x00000000
obj_index:  0x00000008
data:       0x00000001
data_ptr:   0x00000000 0x00000000


BLOBs sess3pkt5 encoding failed
